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BeoSound 2
BeoSound 2 is an elegant and uncomplicated speaker system, designed for a casual 360 degree listening experience. A compelling sound performer enriching your life with its cool presence and minimal fuss.
It offers impressive and omnidirectional sound performance in one single unit that only needs power from the mains to work.
It is seen primarily as a stationary music system, but it can easily be moved around within the home if you have the need. Placement is typically on the floor or a low piece of furniture.

It is an integral part of our BeoLink Multiroom offering which means it can join and playback content from other sources just by a light touch on the top. It works in sync if used with other BeoLink Multiroom products across the room and the house.

You can expand the sound experience by adding more BeoSound 2s in the room or around the house, or you can join in on music played on other devices such as e.g. the smaller BeoSound 1 in another room 
It is based on the new audio engine platform that allows streaming from mobile devices using the latest technologies, such as: AirPlay, Google Cast, DLNA and Bluetooth. At the same time it integrates music services and internet radio  such as: Deezer, TuneIn internet radio, Spotify (Spotify Connect feature) and QQMusic (QPlay feature).
Designer: 

Torsten Valeur, David Lewis Designers
Materials and colour: Anodised and polished natural aluminium
Dimensions and weight:

Diameter: 200 mm - Height: 431 mm

: 
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Weight is 4.1 kg
Acoustic performance
360 degree sound dispersion using Acoustic Lens Technology 

Loudspeaker drivers: 
Active speaker design with

3/4 inch tweeter placed in the top, playing downwards into a reflector for a spherical sound image and a uniform timbre in a 360 degree circumference. 

2 x 2 inch midrange drivers playing through the aluminium grills on the side 

1 x 5 1/4 inch bass driver placed at the bottom of the unit playing downwards allowing us to use a relatively large driver for a great bass performance.  
Power amplifiers:
2 x 20 watts class D for woofer
2 x 11 watts class D for midrange

1 x 40 watts class D for tweeter

Cabinet principle: 
Closed box

Wireless networks:
802.11b/g/n (2.4 GHz & 5GHz) Bluetooth 4.1

Supported 

audio formats: 

MP3, WMA, AAC, ALAC, FLAC, WAV, AIFF

Standard sample rates up to 192 kHz, stereo and up to 24 bit

Includes Bang & Olufsen specific technologies such as Adaptive Bass Linearisation and thermal protection to avoid overload or overheating

Design

Designer: Torsten Valeur, David Lewis designers

Natural anodized, cone shaped cabinet that is slight curved (almost like a trumpet) creates the compact impression that makes the device fit in anywhere on a low table or the floor.

The aluminium cabinet is an extruded tube that is formed in a hydraulic press into the cone shape. The cabinet is 3 mm thick for sufficient stiffness to avoid acoustic vibration and increase the inside space as much as possible to optimise the acoustics. 

The grills at the top are double anodised with black walls and high gloss fronts.

It is lightweight and easy to move around should you decide to use it in another room, all you need is a power outlet nearby.
User interface

On the top of the unit is a capacitive touch sensitive operation wheel where you can swipe between tracks or stations and turn up and down the volume, join or switch off the system. 

An integrated proximity sensor detects where you are coming from, so the operation is always turned in the correct direction for the user regardless of from which direction he or she is approaching the product.  

Swiping is made in the same way you would turn pages in a book – from right to left is swiping forward and from left to right is swiping backwards. 

The top is made in high gloss aluminium with a polished surface with a mechanical volume wheel moving based on a ball bearing design with audible and tactile feedback when turn up or down the volume. You activate BeoSound 1 by pushing at the centre of the surface, and the LED status indicator gives you relevant feedback. 

Connection and operation

1 x Ethernet 10/100 Mbit/s

Besides connector for 230 V mains, there is one connector in the bottom of the speaker holding an RJ45 socket for Ethernet connection used for software updates and one mini-jack socket for line-in connection of external devices e.g. CD player.or the phone, in cases where the wireless performance is insufficient.
BeoSound 2 can be operated with BeoRemote One Bluetooth or via the BeoMusic App, or directly on the device itself, and it can also be paired via the BeoSound Essence Remote.

For more information please contact:

Corporate Communication
Bang & Olufsen a/s

Phone:
+45 96 84 51 00

Bang & Olufsen was founded in Struer, Denmark, in 1925 by Peter Bang and Svend Olufsen, two innovative, young engineers devoted to high quality audio reproduction. Since then, the brand has become an icon of performance and design excellence through its long-standing craftsmanship tradition and the strongest possible commitment to high-tech research and development.

Still at the forefront of domestic technology, Bang & Olufsen has extended its comprehensive experience with integrated audio and video solutions for the home to other areas such as the hospitality and automotive industries in recent years. Consequently, its current product range epitomizes seamless media experiences in the home as well as in the car and on the move.

For more information on Bang & Olufsen, please visit www.bang-olufsen.com.
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